

**MONTHLY AND ANNUAL PERIODIC OPERATION AND MAINTENANCE WALKTHROUGH INSPECTION CHECKLIST**

Louisiana Department of Environmental Quality

Underground Storage Tank Division

|  |  |  |  |
| --- | --- | --- | --- |
| **Facility Name:** |       | **Agency Interest No:** |       |
| **Facility Address:** |       |
|  |
| **UST System Description** **/ List of Areas Checked** (this section must be filled out) |
| **Spill Containment / Spill Buckets** |
| Number Inspected: |    | Describe spill containments with product type in space below, e.g. Regular, Premium, North Tank Regular, South Tank Compartment 1 Premium, Diesel, etc. |
|       |
|       |
|       |
|       |
| **Tank Top / STP Sumps/Areas** |
| Number Inspected: |    | Describe tank top/STP sumps/areas with product type below, e.g. Regular STP sump, Premium STP area, Diesel STP sump, Emergency Generator tank top sump, etc. |
|       |
|       |
|       |
|       |
| **Under-Dispenser Sumps/Areas** |
| Number Inspected: |    | Describe dispenser sumps/areas inspected below, e.g. Dispenser 1/2 sump, Dispenser 3/4 area, Regular UDC sump, Premium dispenser area, Diesel UDC sump, etc. |
|       |
|       |
|       |
|       |
| **Transition Sumps** |
| Number Inspected: |    | Describe transition sumps inspected below, e.g. Regular piping run sump, Diesel/B100 blend unit sump, etc. |
|       |
|       |
|       |
| **Tank Release Detection Type** (Describe tank release detection type below, e.g. ATG, SIR, Interstitial Monitoring (manual or continuous, etc.) |
|       |
|       |
|       |
|       |
| **Piping Release Detection Type** (Describe piping release detection type below, e.g. Annual Line Tightness Test, Monthly with ATG with PLLDs, Monthly with SIR, Monthly Interstitial Monitoring (manual or continuous, etc.) |
|       |
|       |
|       |
|       |
| **REQUIRED MONTHLY (EVERY 30 DAYS)**  |
| **Spill Prevention Equipment** (If your UST system received deliveries at intervals greater than 30 days, you may check your spill prevention equipment prior to each delivery if delivery records are maintained) |
| **Date of Inspection** |       |       |       |       |       |       |
| **Initials of Inspector** |     |     |     |     |     |     |
| Check all spill buckets for damage, cracks, or separation  |   |   |   |   |   |   |
| Check all spill buckets for liquid and debris. Remove all liquid and debris\* |   |   |   |   |   |   |
| Check for and remove obstructions from all fill pipes |   |   |   |   |   |   |
| Check all fill caps to ensure they are secure on the fill pipes |   |   |   |   |   |   |
| For double-walled spill prevention equipment with interstitial monitoring, check for leaks in the interstitial areas |   |   |   |   |   |   |
|  |
| **Release Detection Equipment** |
| **Date of Inspection** |       |       |       |       |       |       |
| **Initials of Inspector** |     |     |     |     |     |     |
| Check all release detection equipment to ensure that there are no alarms or unusual operating conditions |   |   |   |   |   |   |
| Review and confirm release detection records are current |   |   |   |   |   |   |
|  |
| **REQUIRED ANNUALLY (EVERY 365 Days)** |
| **Date of Inspection** |       |       |       |       |       |       |
| **Initials of Inspector** |     |     |     |     |     |     |
| **Containment Sumps Installed After 12/20/08 and Containment Sumps Used For Interstitial Monitoring** |
| Visually check all containment sumps for damage to sumps and to equipment within the sumps  |   |   |   |   |   |   |
| Visually check for leaks to the containment area |   |   |   |   |   |   |
| Visually check for releases to the environment |   |   |   |   |   |   |
| Remove liquid and debris from containment sumps\* |   |   |   |   |   |   |
| For double-walled containment sumps with interstitial monitoring, check for leaks in the interstitial areas |   |   |   |   |   |   |
|  |
| **Containment Sumps Installed Before 12/20/08 That Are Not Used For Interstitial Monitoring** |
| Visually check all containment sumps for damage to equipment within the sumps |   |   |   |   |   |   |
| Visually check for releases in the containment sumps and to the environment |   |   |   |   |   |   |
| Visually check for the presence of cathodic protection if the sumps contain water that is in contact with metal components that routinely contain product  |   |   |   |   |   |   |
| Remove any debris from containment sumps\* |   |   |   |   |   |   |
|  |
| **Submersible Turbine Pump Areas and Under-Dispenser Areas That Do Not Have Containment Sumps** |
| Visually check for damage to equipment within the areas |   |   |   |   |   |   |
| Visually check for releases to the environment |   |   |   |   |   |   |
| Visually check for the presence of cathodic protection if any metal components that routinely contain product are in contact with soil, backfill, or water |   |   |   |   |   |   |
| Remove any debris\* |   |   |   |   |   |   |
|  |
| **Hand-Held Release Detection Equipment** |
| **Date of Inspection** |       |       |       |       |       |       |
| **Initials of Inspector** |     |     |     |     |     |     |
| Check all devices (e.g. tank gauge sticks, groundwater bailers) for operability and serviceability |   |   |   |   |   |   |
|  |
| **Describe Actions Taken To Correct Issues Discovered** (must list specific UST component action applies to) |
| **Date** | **Action Taken** |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |

\* Removed liquid and debris must be properly managed and/or disposed properly

* + Petroleum-contaminated liquid and debris can be reclaimed by a fuel recycling facility
	+ Petroleum-contaminated liquid and debris can be disposed (Solid and Hazardous Waste rules apply and the waste must be characterized and managed appropriately)

Walkthrough inspection records must be maintained for 3 years.